{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["Sheet4","Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":42},"read":"whole","date_system":"1900"}

{"sheet":"Sheet4","index":0,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet2","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":3,"n_rows":62,"n_cols":17,"rows_kept":62}
[]
[null,"FIXED_DUTY 모드",{"$nulls":8},"LulSclClkGenDiv = 0"]
[{"$nulls":10},"LddChannel = 5"]
[{"$nulls":10},"LulICCCRegVal = 30"]
[{"$nulls":10},"LulICCCReg2Val = 128"]
[]
[]
[]
[]
[]
[{"$nulls":10},"pICCCRnReg","->","LulICCCRegVal = 30"]
{"$rows_empty":7}
[{"$nulls":10},"pICCCR2nReg",null,"LulICCCReg2Val = 128"]
{"$rows_empty":7}
[{"$nulls":10},"pICFBSCRnReg",null,"LpSlaveConfig->ucFisrtBitSetupCycle = 13"]
{"$rows_empty":7}
[{"$nulls":10},"SCLfreq = I2Cck / (20 + SCGD × 8 + F[(tICF + tr + IntDelay) × I2Cck])"]
[{"$nulls":10},"SCLfreq: 실제 I2C SCL 클럭 주파수(Hz)"]
[{"$nulls":10},"I2Cck: I2C 컨트롤러에 공급되는 내부 클럭(19MHz)"]
[{"$nulls":10},"SCGD: I2C 클럭 분주 레지스터 값(3, Tr32로 Register를 확인함)"]
[{"$nulls":10},"tICF: SCL의 실제 하강(fall) 시간(ns)"]
[{"$nulls":10},"tr: SCL의 실제 상승(rise) 시간(ns)"]
[{"$nulls":10},"IntDelay: LSI(내부 논리) 지연시간 (Open Drain Buffer: 50ns typ, 110ns max)"]
[{"$nulls":10},"F[...]: 괄호 안 값을 반올림(혹은 내림) 함수로 처리"]
[]
[{"$nulls":9},"DaVinci","계산식"]
[{"$nulls":10},"SCLfreq",{"$f":"L46/(20+L47*8+ROUNDDOWN((L48+L49+L50)*L46/1000000000,0))/1000","v":422.22222222222223},"KHz"]
[{"$nulls":10},"I2Cck",19000000,"Hz"]
[{"$nulls":10},"SCGD",3,null,{"$f":"L48+L49+L50","v":56},"ns",{"$f":"N47/1000000000","v":5.6e-08},"s"]
[{"$nulls":9},"Iic Falling Time","tICF",3,"ns",{"$f":"P47*L46","v":1.064}]
[{"$nulls":9},"Iic Rising Time","tr",3,"ns",{"$f":"ROUNDDOWN((L48+L49+L50)*L46/1000000000,0)","v":1}]
[{"$nulls":9},"Iic Inbt Delay","IntDelay",50,"ns"]
[]
[{"$nulls":10},"Target scl은 왜 필요하지?"]
[]
[]
[]
[{"$nulls":10},"SCLfreq: 실제 I2C SCL 클럭 주파수(Hz)"]
[{"$nulls":10},"I2Cck: I2C 컨트롤러에 공급되는 내부 클럭(19MHz)"]
[{"$nulls":10},"SCGD: I2C 클럭 분주 레지스터 값(3, Tr32로 Register를 확인함)"]
[{"$nulls":10},"tICF: Iic Falling Time(ns)"]
[{"$nulls":10},"tr: Iic Rising Time(ns)"]
[{"$nulls":10},"IntDelay: Iic Inbt Delay (Open Drain Buffer: 50ns typ, 110ns max)"]
[{"$nulls":10},"F[...]: 괄호 안 값을 반올림(혹은 내림) 함수로 처리"]