{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["회로","파형 및 Source"],"not_rendered":{"images":7},"read":"whole","date_system":"1900"}

{"sheet":"회로","index":0,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"파형 및 Source","index":1,"n_rows":85,"n_cols":5,"rows_kept":85}
[]
[null,null,"초음파(MSIOF1)","EEPROM(MSIOF4)","ADC(MSIOF5)"]
{"$rows_empty":59}
[null,null,"#define PFC_MCU_BASE    (uint32)0xE6050000UL","#define PMMR1              *((volatile uint32 *)(PFC_MCU_BASE + PFC_PORT_GRP1 + 0x0000U))","#define PMMR0              *((volatile uint32 *)(PFC_MCU_BASE + PFC_PORT_GRP0 + 0x0000U))"]
[null,null,"#define PFC_PORT_GPR1   (0x00000800UL)  /* Port Group1 */"]
[null,null,"#define PFC_RW_OFFSET   (uint32)0x00000000UL","#define PFC_DRV3CTRL1_RW   *((volatile uint32 *)(PFC_MCU_BASE + PFC_PORT_GRP1 + PFC_RW_OFFSET + 0x008CU))","#define PFC_DRV0CTRL0_RW   *((volatile uint32 *)(PFC_MCU_BASE + PFC_PORT_GRP0 + PFC_RW_OFFSET + 0x0080U))"]
[null,null,"#define PFC_DRV0CTRL1_RW   *((volatile uint32 *)(PFC_MCU_BASE + PFC_PORT_GRP1 + PFC_RW_OFFSET + 0x0080U))","#define PFC_DRV2CTRL1_RW   *((volatile uint32 *)(PFC_MCU_BASE + PFC_PORT_GRP1 + PFC_RW_OFFSET + 0x0088U))","#define PFC_DRV1CTRL0_RW   *((volatile uint32 *)(PFC_MCU_BASE + PFC_PORT_GRP0 + PFC_RW_OFFSET + 0x0084U))"]
[null,null,"#define PFC_DRV0CTRL1_RW_ADD   (PFC_MCU_BASE + PFC_PORT_GRP1 + PFC_RW_OFFSET + 0x0080U)"]
[{"$nulls":3},"#define PFC_DRV3CTRL1_RW_ADD   (PFC_MCU_BASE + PFC_PORT_GRP1 + PFC_RW_OFFSET + 0x008CU)","#define PFC_DRV0CTRL0_RW_ADD   (PFC_MCU_BASE + PFC_PORT_GRP0 + PFC_RW_OFFSET + 0x0080U)"]
[null,null,"#define PMMR1   *((volatile uint32 *)(0xE6050800UL))","#define PFC_DRV2CTRL1_RW_ADD   (PFC_MCU_BASE + PFC_PORT_GRP1 + PFC_RW_OFFSET + 0x0088U)","#define PFC_DRV1CTRL0_RW_ADD   (PFC_MCU_BASE + PFC_PORT_GRP0 + PFC_RW_OFFSET + 0x0084U)"]
[null,null,"  volatile uint32 *regval;"]
[null,null,"#endif","PMMR1 = ~(PFC_DRV3CTRL1_RW & ~((uint32)0x00077777));","PMMR0 = ~(PFC_DRV0CTRL0_RW & ~((uint32)0x70000000));"]
[{"$nulls":3},"regval = (volatile uint32 *)PFC_DRV3CTRL1_RW_ADD;","regval = (volatile uint32 *)PFC_DRV0CTRL0_RW_ADD;"]
[{"$nulls":3},"*regval = (PFC_DRV3CTRL1_RW & ~((uint32)0x00077777));","*regval = (PFC_DRV0CTRL0_RW & ~((uint32)0x70000000));"]
[]
[{"$nulls":3},"PMMR1 = ~(PFC_DRV3CTRL1_RW | ((uint32)0x00011111));","PMMR0 = ~(PFC_DRV0CTRL0_RW | ((uint32)0x10000000));"]
[{"$nulls":3},"regval = (volatile uint32 *)PFC_DRV3CTRL1_RW_ADD;","regval = (volatile uint32 *)PFC_DRV0CTRL0_RW_ADD;"]
[{"$nulls":3},"*regval = (PFC_DRV3CTRL1_RW | ((uint32)0x00011111));","*regval = (PFC_DRV0CTRL0_RW | ((uint32)0x10000000));"]
[]
[]
[null,null,"PMMR1 = ~(PFC_DRV0CTRL1_RW & ~((uint32)0x00777700));","PMMR1 = ~(PFC_DRV2CTRL1_RW & ~((uint32)0x70000000));","PMMR0 = ~(PFC_DRV1CTRL0_RW & ~((uint32)0x00077777));"]
[null,null,"regval = (volatile uint32 *)PFC_DRV0CTRL1_RW_ADD;","regval = (volatile uint32 *)PFC_DRV2CTRL1_RW_ADD;","regval = (volatile uint32 *)PFC_DRV1CTRL0_RW_ADD;"]
[null,null,"*regval = (PFC_DRV0CTRL1_RW & ~((uint32)0x00777700));","*regval = (PFC_DRV2CTRL1_RW & ~((uint32)0x70000000));","*regval = (PFC_DRV1CTRL0_RW & ~((uint32)0x00077777));"]
[]
[null,null,"PMMR1 = ~(PFC_DRV0CTRL1_RW & ~((uint32)0x00333300));","PMMR1 = ~(PFC_DRV2CTRL1_RW | ((uint32)0x10000000));","PMMR0 = ~(PFC_DRV1CTRL0_RW | ((uint32)0x00011111));"]
[null,null,"regval = (volatile uint32 *)PFC_DRV0CTRL1_RW_ADD;","regval = (volatile uint32 *)PFC_DRV2CTRL1_RW_ADD;","regval = (volatile uint32 *)PFC_DRV1CTRL0_RW_ADD;"]
[null,null,"*regval = (PFC_DRV0CTRL1_RW & ~((uint32)0x00333300));","*regval = (PFC_DRV2CTRL1_RW | ((uint32)0x10000000));","*regval = (PFC_DRV1CTRL0_RW | ((uint32)0x00011111));"]